OFFER FOR MARKET RESEARCH
REPAIR OF TRAM 15T BOGIE FRAMES
Date: __.______ 2026
1. SUBMITED BY
	Company name*
	

	Company registration number
	


*Hereinafter - Applicant
2. CONTACT PERSON
	Name, surname, position
	

	Phone number
	

	Email address
	


MARKET RESEARCH TERMS

2.1. The subject matter of market research is inspection of bogie frames and wheelset frames of Škoda 15T, 15T1, 15T2 and 15T2A trams using the magnetic particle testing (MT) method as well as their repair in accordance with the requirements of the Technical Specification (hereinafter collectively referred to as the “Service”).
2.2. The purpose of this market research is to conclude a contract for the subject matter of the market research.
2.3. When evaluating the offers, the Contracting Authority shall have the right to request additional information regarding the offer, the proposed Service, and the experience and qualifications of the Applicant and the specialists proposed by the Applicant.
2.4. When evaluating the Applicant’s offer, the Contracting Authority shall verify the offer’s compliance with the requirements set out in the Market research terms and, among the offers that comply with these requirements, select the offer in accordance with the specified evaluation criterion.
2.5. The offer evaluation criterion is the lowest-price offer.
2.6. The Contracting authority has the right to suspend or terminate the market research without results.
2.7. The Contracting Authority shall have the right to correct arithmetic errors identified during the evaluation of the offers, informing the Applicant of all such corrections. Arithmetic errors shall be corrected in the following order:
2.7.1. When recalculating the Applicant’s financial offer, the calculation shall be made based on the unit prices specified in the offer signed by the Applicant.
2.7.2. When evaluating and comparing offers containing arithmetic errors, the Contracting Authority shall take into account only the corrected prices.
2.8. The Contracting Authority reserves the right to verify compliance with the qualification requirements only for the Applicant whose offer has the lowest total offered price, after verifying that the financial offer does not contain any arithmetic errors.
2.9. During the market research, the Contracting Authority may conduct negotiations with the Applicants. During the negotiations, the Contracting Authority may request the Applicants to clarify their offers and to supplement or improve their offers. Please indicate whether the Applicant agrees to this condition by selecting one of the following options: 
☐	Yes
☐	No
2.10. The Contracting Authority shall have the right to reject an Applicant’s offer if, during the three years preceding the date of announcement of the market research[footnoteRef:2], the Applicant, its member or partner (if the Applicant is a consortium or partnership), as a contracting party or a member or partner of a contracting party (if the contracting party was a consortium or partnership), failed to properly perform a procurement contract, framework agreement or order placed without concluding a procurement contract with the Contracting Authority, and as a result of such failure, any of the following circumstances occurred: [2:  If a procurement contract with the Applicant was concluded for a period exceeding three years and the market research concerns the same subject matter, the Contracting Authority shall be entitled to take into account the quality of performance of such contract.] 

· the right to terminate the contract unilaterally arose, regardless of whether this right was actually exercised; 
· an obligation to compensate for damages arose; 
· the Contracting Authority imposed contractual penalties for systematic breaches of the contractual requirements, indicating significant deficiencies in contract performance.
3. APPLICANT’S DECLARATION
3. We hereby declare that the Applicant is not insolvent, is not undergoing liquidation, its business activities have not been suspended, it has no tax debts exceeding EUR 150.00, and it has not been removed from the Register of Value Added Tax Payers (if the entity is a Value Added Tax payer).
3. The Applicant is not subject to the exclusion grounds referred to in Section 11.1, Paragraphs 1 and 2 of the Law on International Sanctions and National Sanctions of the Republic of Latvia.
3.2. We certify that the Applicant is not subject to the restrictions set out in Council Regulation (EU) 2025/2033 of 23 October 2025 amending Regulation (EU) No 833/2014 concerning restrictive measures in view of Russia’s actions destabilising the situation in Ukraine, Article 5k(1), namely that neither the Applicant nor its subcontractors are:
a) 	a Russian national or a natural person residing in Russia, or a legal person, entity or body established in Russia;
b) a legal person, entity or body whose proprietary rights are directly or indirectly owned for more than 50% by a person or entity referred to in point (a); or 
c) a natural or legal person, entity or body acting on behalf of or at the direction of an entity referred to in points (a) or (b),
d) including subcontractors, suppliers or entities whose capacities are relied upon within the meaning of the public procurement directives where their involvement exceeds 10% of the contract value.
3.3. The submitted financial offer includes all costs related to the provision of the Service to the Contracting Authority in accordance with the requirements set out in the Technical Specification and the Financial Offer Form.
3.4. The validity period of the offer is 60 (sixty) days from the deadline for submission of offers.
3.5. We confirm that we have reviewed the Technical Specification and consider it to be:
☐	Executable and its content is sufficient to submit an offer;
☐	Requiring improvement:________________________________________
	If you noted that the technical specification needs improvement, please indicate what exactly needs to be improved or what information is unclear in order to prepare an offer.
We encourage you to submit any questions or requests for clarification before submitting your offer.


3.6. Attracting subcontractors (if planned):
☐	We confirm that we will perform the contract independently, without involving subcontractors.
☐	It is planned to involve subcontractors (including self-employed persons) in the execution of the contract :
	No
	Name and registration number/ first name, last name
	Submittable work assignments
	Transferable portion of contract amount (EUR)
	Does the Applicant rely on the capacities of a subcontractor?

	
	
	
	
	☐ Yes, on the economic and financial standing;
☐ Yes, on the technical and professional capacity;
☐ No



3.7. [bookmark: _Hlk210114136]The Applicant has experience, during the last 3 (three) years (2023, 2024, 2025 and 2026 up to the date of submission of the offer), in the performance of at least 2 (two) contracts involving the processing of metal components by shot blasting, metallization and painting.
	No
	Customer, contact details, address
	Description of the services demonstrating compliance with the requirement set out in Clause 4.8
	Contract performance period (from- to)

	1.
	
	
	

	2.
	
	
	


3.8. The Applicant shall ensure the performance of magnetic particle testing (MT) by providing documents demonstrating the competence and authorization of the Applicant or its engaged service provider to perform such testing.
3.9. The Applicant may rely on the capacities of other entities to demonstrate the Applicant’s compliance with the qualification requirements set out in Clauses 4.8 and 4.9.[footnoteRef:3] In such case, the Applicant shall demonstrate to the Contracting Authority that the necessary resources will be available to the Applicant by submitting an undertaking from such entity or an agreement concerning the provision of the necessary resources to the Applicant. [3:  The Applicant may rely on the capacities of other entities only if such entities will perform the services for which the respective capacities are required.] 

	No
	Name and registration number/ first name, last name
	Description of the capacities on which the Applicant relies

	
	
	


4. FINANCIAL OFFER AND SERVICE DELIVERY PERIOD
4.1. The Applicant shall submit an offer by completing the Financial Offer Form (Annex 2).
4.2. When submitting the Financial Offer, the Applicant shall indicate the offered prices with an accuracy of up to two decimal places.
4.3. The estimated contract term: 6 (six) months.
4.4. Payment terms: within 30 (thirty) calendar days of receipt of the invoice.
4.5. Expected place of contract performance (place of provision of the Services): [Please indicate the address where the Services will be provided]: ______________.
4.6. Other conditions ensuring the validity of the offered price:
Please specify any other conditions, if applicable, that the Contracting Authority should take into account to ensure that the offer remains valid at the stated price.
5. CONTACT INFORMATION
Upon request, additional information will be provided by Contacting Authorities’ contact person: Procurement and Contract Management Department , Procurement Specialist, Market Research and Procurement Methodology Department, Nataļja Vjatkina, by sending the request to the e-mail: natalja.vjatkina@rigassatiksme.lv
6. INFORMATION ABOUT THE CONTRACTING AUTHORITY 
Limited Liability Company “Rīgas satiksme” was founded on February 20, 2003. „Rīgas satiksme” is a company with share capital 100% owned by Riga city municipality. The company operates in conformity with internationally recognized standards: ISO 9001:2015 quality management system, ISO 45001:2018 occupational health and safety management system, as well as ISO 50001:2018 energy management system ( https://www.rigassatiksme.lv/lv/par-mums/publiskojama-informacija/sertifikati/ ).
ANNEX:
Annex 1 “Technical Specification”.
Annex 2 “Financial Offer Form” ( excel file ).



Annex 1
TECHNICAL SPECIFICATION
	REPAIR OF TRAM 15T BOGIE FRAMES

	1. 1
	In order to ensure safe and uninterrupted operation of Škoda 15T, 15T1, 15T2 and 15T2A trams, it is necessary to carry out inspection of bogie frames and wheelset frames (hereinafter – Parts) using the magnetic particle inspection method.
	

	1. 2
	The financial offer shall be submitted for TR1, TR2, TR3 bogie frames and wheelset frames.
	

	1. 3
	If the work cannot be fully completed, the Customer shall issue an invoice for the work actually performed.
	

	1. 5
	In case of references to standards used in the Technical Specification, the latest version of the standard shall apply.
	

	1. 6
	Quantity of Parts subject to repair: TR1 – 3 pcs; TR2 – 6 pcs; TR3 – 3 pcs; wheelset frames – 24 pcs.
	

	1. 7
	Contract execution period: 6 months.
	


	1. 
	The work completion period is 1 month from the date of receipt of the bogie frames. The quantity per shipment shall not exceed 3 sets of frames (3 bogie frames and 6 wheelset frames).
	

	1. 8
	The price shall include all costs related to service provision, materials, personnel remuneration, taxes and duties (excluding VAT), permits from third parties, and other expenses necessary to ensure full performance of the service in accordance with the Technical Specification.
	

	1. 9
	Transportation services to and from the repair site shall be provided by the Customer using its own technical resources and at its own expense, except in cases where the Contractor’s proposed transportation costs are lower and more economically advantageous for the Customer.
	



	1. TECHNICAL SPECIFICATION for repair works

	No.
	Name of technological operation
	Specific requirements
	Notes

	

	9.1
	Transportation of parts from the Customer to the Contractor and back.
	The Customer hands over to the Contractor and receives from the Contractor the parts in a disassembled condition (i.e. the bogie frame and the wheelset frame separately).
	Address for issuing and receiving the parts: 5th Depot, 191 Brīvības Street, Riga. Delivery of the parts to/from the place of service provision shall be at the Customer’s technical and financial expense.

	9.2
	Supplied Parts Package
	One set consists of: 1 bogie frame and 2 wheelset frames
	

	9.3
	Frame geometry inspection
	Inspect the bogie and bridge frames in accordance with the technical documentation.
	The Contractor shall inform the Contracting Authority of any identified non-conformities.

	9.4
	Protective covers for parts
	The quantity and type of protective covers are specified in drawings– 0833001105, 0833001106,0833000078, 0833000088.
	The customer provides the protective covers shown in the drawings for the performance of the work.

	9. 5
	Shot blasting of parts
	Complete cleaning of parts from paint and metallization layer. After shot blasting, ensure that the average roughness of the treated surface corresponds to Ra ≤ 6.3 µm.
	1. Before installing the protective covers, clean and re-tap the frame threads. Cut off the wire fasteners. Cover the frame identification plate so that it remains legible after processing. 
1. Install protective covers , fasteners and cover threads for TR1 frame according to drawing 0833001105, for TR2 frame drawing 0833001106, for TR3 frame drawing 0833000088, for Bridge frame 0833000078 page 1.
1. The surfaces covered with protective covers must not be damaged as a result of processing parts .
1. Processing of the parts shall not affect the results of magnetic particle inspection.

	9.6
	Magnetic Particle Inspection and Its Results
	1. Inspection points: 
1.1. Wheelset frame (drawing No. D0535327 1., 2. and 3. page): 
- welded joints, EN 1290 and EN 1291 grade 2X;
 -  as-cast surfaces, EN ISO 9934-1 and EN 1369 quality level LM01, AM01, SM01;
 - machined cast surfaces, EN ISO 9934-1 and EN 1369 quality level LM001, AM001, SM00
1.1.2. Front bogie frame (drawing No. D0582573), middle bogie frame (drawing No. D0582590), rear bogie frame (drawing No. D0582620):
-inspection shall be carried out in accordance with ISO/TS 18173 and EN ISO 9934-1 standards;
-welded joints, EN 1290 and EN 1291 grade 2X.
2. The inspection shall be carried out in accordance with the requirements of EN ISO 9712. A defect inspection report shall be prepared as a result of the inspection. 
3. If defects in the wheelset frame are located outside the weld seam, repair is permitted provided that the crack depth does not exceed 5 mm and the crack length does not exceed 20 mm.
4. For the bogie frame, the maximum permissible size of an isolated defect in an as-cast area is 3 mm.
5. Grinding is permitted at locations no closer than 20 mm from the weld seam. 
6. The maximum permissible reduction in material thickness is 10% of the nominal material thickness specified in the manufacturing documentation.
	1. Remove the protective covers before inspection.
2. The inspection is carried out based on the aforementioned standards or other applicable standards that replace those specified in the specific requirements. In the event that the standards are changed, the Contractor shall submit them to the Customer.
3. A separate defect inspection report shall be prepared for each frame, indicating the frame number and drawing number. If an indication is detected, its location shall be marked on the drawing and an image shall be attached.

	
	
	
	
	

	
	
	
	
	

	9.6.1
	
	No unacceptable indications are detected.
	
	

	9.6.2
	
	Casting indications are detected, removed by grinding, and are no longer detected upon repeated inspection.
	
	

	9.6.3
	
	Unacceptable indications are detected that remain after grinding – no further processing shall be carried out, and the frame shall be returned to the Customer together with the defect inspection report.
	
	

	9.7
	Shot Blasting (Preparation for Metallization)
	Before metallization, the surface shall be cleaned of magnetic particle inspection residues and other contaminants by shot blasting to Sa2 in accordance with ISO 8501.
	Install protective covers, fasteners and cover the threads for the TR1 frame in accordance with drawing 0833001105, for the TR2 frame in accordance with drawing 0833001106, for the TR3 frame in accordance with drawing 0833000088, and for the Bridge frame in accordance with drawing 0833000078, page 1. 
	

	9.8
	Metallization
	1. Metallization should be carried out no later than 4 hours after shot blasting. 
2. Metallization layer thickness: ≥80µm. 3. Metallization material: zinc aluminum 85/15 wire.
	Install protective covers, fasteners and cover the threads for the TR1 frame in accordance with drawing 0833001105, for the TR2 frame in accordance with drawing 0833001106, for the TR3 frame in accordance with drawing 0833000088, and for the Bridge frame in accordance with drawing 0833000078, page 1. 
	

	9.9
	Painting
	1. 2K polyurethane-based primer, dry film thickness ≥90 µm, grey; 
2. 2K polyurethane-based paint, dry film thickness ≥80 µm, RAL 7021.
	Install protective covers, fasteners and cover the threads for the TR1 frame in accordance with drawing 0833001105-01, for the TR2 frame in accordance with drawing 0833001106-01, for the TR3 frame in accordance with drawing 0833000088-01, and for the Bridge frame in accordance with drawing 0833000078, page 2. 
	

	9.10
	Preparation of the Bogie for Shipment
	Prepare defect inspection reports and the acceptance and handover report for the dispatched bogie shipment. Remove the covers from untreated surfaces (shot-blasted, metallized and painted areas) and preserve them using Tectyl 506, CRC SP-400, Dinitrol 4941 or an equivalent product.
	
	

	9.11
	Documentation
	A document confirming a 12-month warranty for the completed work and a summary of the quality characteristics of the materials used (for paint, galvanization, etc. – protection class of the treated surface and material data for the metallization process)
	 
 
	



Appendix 1 – Technical Documentation of the Bogie Frames (provided as a separate appendix).
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