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07.08.2026.


Par iepirkumu procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) nolikuma prasībām

Rīgas pašvaldības sabiedrības ar ierobežotu atbildību „Rīgas satiksme” (turpmāk – Pasūtītājs) Iepirkuma komisija no iespējamā pretendenta ir saņēmusi lūgumu sniegt atbildes uz jautājumiem par iepirkuma procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) (turpmāk – iepirkuma procedūra) nolikuma prasībām.

1.jautājums
Vēlamies precizējumus par atklāta konkursa “Autobusu piegāde” Identifikācijas Nr.: RS/2026/17. 
Ņemot vērā, ka sistēmas ir identiskas, tad šie jautājumi attiecas uz: 
18m elektroautobusiem; 
18m dīzeļu autobusiem. 

Lūdz precizēt Tehniskās specifikācijas 9.7.2. punktā noteiktās prasības attiecībā uz Ethernet tīkla komutatoriem (switchiem) ar PoE funkcionalitāti. 
Tehniskajā specifikācijā ir noteikts, ka: 
"Transportlīdzeklī jāparedz vieta Ethernet tīkla komutatoriem ar vismaz 16 brīviem portiem un PoE funkciju. Komutatorus nodrošina Pasūtītājs, bet transportlīdzeklī uzstāda Piegādātājs." 
Vienlaikus specifikācijā nav norādītas prasības, kas nepieciešamas transportlīdzekļa elektroinstalācijas un komunikāciju infrastruktūras projektēšanai. 
Lūdzam precizēt šādu informāciju: 
1. Kāds PoE standarts tiks izmantots Pasūtītāja piegādātajiem Ethernet komutatoriem (IEEE 802.3af, IEEE 802.3at (PoE+), IEEE 802.3bt vai cits)? 
2. Vai Ethernet komutatori būs aprīkoti ar RJ45 vai M12 Ethernet pieslēgvietām, vai arī ir paredzēts cits savienotāju risinājums? 
3. Kāda ir paredzētā maksimālā PoE jauda uz vienu portu un kopējais komutatora PoE jaudas budžets (Power Budget)? 
5. Vai Pasūtītāja piegādātie Ethernet komutatori būs pārvaldāmi (Managed) vai nepārvaldāmi (Unmanaged)? 
Šī informācija ir būtiska, lai autobusa ražotājs varētu pareizi izprojektēt komunikāciju infrastruktūru, izvēlēties piemērotus savienotājus, kabeļus, montāžas risinājumus un nodrošināt pilnīgu transportlīdzekļa atbilstību tehniskās specifikācijas prasībām.

Atbilde:
Pasūtītājs skaidro, ka Tehniskajā specifikācijas 9.7.2. punktā "Lokālais datu tīkls" ir prasība - "Transportlīdzeklī jāparedz vieta Ethernet tīkla komutatoriem ar vismaz 16 brīviem portiem un PoE funkciju".
Informācija par:(1)PoEstandartu, (2) par to Ethernet pieslēgvietām, par (3) maksimālo PoE jaudu un (4) vai Pasūtītāja piegādātie Ethernet komutatori būs pārvaldāmi (Managed) vai nepārvaldāmi (Unmanaged) - neattiecas uz šo iepirkuma procedūru un nav nepieciešama piedāvājuma sagatavošanai. Attiecīgā informācija būs zināma tikai tad, kad Pasūtītājs pabeigs atsevišķu iepirkuma procedūru par attiecīgā aprīkojuma iegādi.



2.jautājums
Lūgums precizēt Ethernet komutatoru (PoE switchu) prasības 
Lūdzam precizēt Tehniskās specifikācijas prasības attiecībā uz Ethernet tīkla komutatoriem (PoE switchiem), jo, izvērtējot 9. nodaļas prasības kopumā, nav viennozīmīgi saprotams to piegādes un funkcionalitātes sadalījums. 
Piemēram, 9.4.1. punktā (Videokameras) ir noteikts, ka pie katras kameras montāžas vietas jānodrošina PoE barošana un Ethernet Cat6 pieslēgums, kas izbūvēts no 9.7.2. punktā minētajiem Ethernet tīkla komutatoriem. Savukārt 9.7.2. punktā ir noteikts, ka Ethernet komutatorus ar PoE funkciju nodrošina Pasūtītājs, bet tos transportlīdzeklī uzstāda Piegādātājs. 
Vienlaikus Pasažieru informācijas sistēmai (PIS), APC un citām Ethernet tīklā integrētajām sistēmām tehniskajā specifikācijā ir paredzēti Ethernet pieslēgumi, tomēr nav skaidrs, vai: 
- visas Ethernet iekārtas (PIS, APC, CCTV u.c.) ir paredzēts pieslēgt tikai Pasūtītāja piegādātajiem Ethernet komutatoriem; 
- vai arī autobusa piegādātājs drīkst vai tam ir jāizmanto papildu Ethernet komutatori savu sistēmu darbības nodrošināšanai. 
Lūdzam precizēt: 
1. Vai visi Ethernet tīkla komutatori transportlīdzeklī, tostarp PoE komutatori, tiks nodrošināti tikai no Pasūtītāja puses? 
2. Vai autobusa piegādātājam ir atļauts vai nepieciešams uzstādīt papildu Ethernet komutatorus (piemēram, Pasažieru informācijas sistēmas vajadzībām), vai arī visas Ethernet iekārtas obligāti jāpievieno tikai Pasūtītāja piegādātajiem komutatoriem? 
Šāds precizējums ir būtisks, lai korekti izstrādātu transportlīdzekļa komunikāciju tīkla arhitektūru un nodrošinātu atbilstību tehniskās specifikācijas prasībām.

Atbilde:
Par jautājuma 1.sadaļu:
Pasūtītājs apstiprina, ka minētie  Ethernet tīkla komutatori transportlīdzeklī, tostarp PoE komutatori, tiks nodrošināti no Pasūtītāja puses.
Par jautājuma 2.sadaļu:
Pasūtītājs norāda, ka nav atļauts un nav nepieciešams uzstādīt papildu Ethernet komutatorus. Visas Ethernet iekārtas obligāti jāpievieno tikai Pasūtītāja piegādātajiem komutatoriem.



Iepirkuma komisijas priekšsēdētāja vietniece
										L. Hodaseviča  




07.08.2026.


Regarding the requirements of the open procedure "Supply of buses" (ID No RS 2026/17)

Riga Municipality Limited Liability Company (SIA) Rīgas satiksme (hereinafter – the Contracting Authority) has received a request from a potential Tenderer to provide answers to questions concerning the requirements of the Regulations of the open procedure "Supply of buses" (ID No RS 2026/17) (hereinafter – the procurement procedure).

Question 1
We would like to request clarifications regarding the open tender “Supply of Buses”, Identification No. RS/2026/17.
Considering that the systems are identical, these questions apply to:
· 18 m electric buses;
· 18 m diesel buses.
We kindly request clarification of the requirements set out in Section 9.7.2 of the Technical Specification regarding Ethernet network switches with PoE functionality.
The Technical Specification states that:
“The vehicle shall provide installation space for Ethernet network switches with at least 16 free ports and PoE functionality. The switches shall be provided by the Contracting Authority, but installed in the vehicle by the Supplier.”
At the same time, the specification does not define the requirements necessary for the design of the vehicle's electrical installation and communication infrastructure.
We kindly request clarification of the following information:
1. Which PoE standard will be used by the Ethernet switches supplied by the Contracting Authority (IEEE 802.3af, IEEE 802.3at (PoE+), IEEE 802.3bt, or another standard)?
2. Will the Ethernet switches be equipped with RJ45 or M12 Ethernet ports, or is another connector solution envisaged?
3. What is the maximum PoE power per port and the total PoE power budget of the switch?
4. What are the power supply requirements for the Ethernet switches (supply voltage range, nominal power consumption, peak power consumption)?
5. Will the Ethernet switches supplied by the Contracting Authority be managed or unmanaged switches?
This information is essential to enable the bus manufacturer to properly design the communication infrastructure, select appropriate connectors, cables and mounting solutions, and ensure full compliance of the vehicle with the requirements of the Technical Specification.
(Translated from Latvian using the machine translation tool “Copilot”)

Answer: 
The Contracting Authority clarifies that Section 9.7.2 “Local Data Network” of the Technical Specification contains the requirement that “the vehicle shall provide installation space for Ethernet network switches with at least 16 free ports and PoE functionality”.
Information regarding: (1) the PoE standard, (2) the type of Ethernet ports, (3) the maximum PoE power, and (4) whether the Ethernet switches supplied by the Contracting Authority will be managed or unmanaged, is not relevant to this procurement procedure and not necessary for the preparation of a tender. The relevant information will only be known once the Contracting Authority has completed a separate procurement procedure for the acquisition of the respective equipment.

Question 2
Request for clarification of Ethernet switch (PoE switch) requirements
We kindly request clarification of the Technical Specification requirements regarding Ethernet network switches (PoE switches), as, upon reviewing the requirements of Section 9 as a whole, the allocation of supply responsibilities and functionality is not unambiguously clear.
For example, Section 9.4.1 (Video Cameras) stipulates that PoE power supply and an Ethernet Cat6 connection originating from the Ethernet network switches referred to in Section 9.7.2 must be provided at each camera mounting location. At the same time, Section 9.7.2 states that Ethernet switches with PoE functionality shall be provided by the Contracting Authority, while their installation in the vehicle shall be performed by the Supplier.
At the same time, the Technical Specification provides for Ethernet connections for the Passenger Information System (PIS), APC and other systems integrated into the Ethernet network; however, it is unclear whether:
· all Ethernet devices (PIS, APC, CCTV, etc.) are intended to be connected only to the Ethernet switches supplied by the Contracting Authority; or
· the bus supplier is permitted or required to use additional Ethernet switches to ensure the operation of its own systems.
We kindly request clarification of the following:
1. Will all Ethernet network switches in the vehicle, including PoE switches, be supplied solely by the Contracting Authority?
2. Is the bus supplier permitted or required to install additional Ethernet switches (for example, for the purposes of the Passenger Information System), or must all Ethernet devices be connected exclusively to the switches supplied by the Contracting Authority?
Such clarification is essential to ensure the proper design of the vehicle communication network architecture and compliance with the requirements of the Technical Specification.
(Translated from Latvian using the machine translation tool “Copilot”)

Answer: 
Regarding Section 1 of the question:
The Contracting Authority confirms that the aforementioned Ethernet network switches in the vehicle, including PoE switches, will be supplied by the Contracting Authority.

Regarding Section 2 of the question:
The Contracting Authority states that the installation of additional Ethernet switches is neither permitted nor required. All Ethernet devices must be connected exclusively to the switches supplied by the Contracting Authority.



Deputy Chairperson of the Procurement Commission
										L. Hodaseviča 
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