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11.08.2026.
 

Par iepirkumu procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) nolikuma prasībām

Rīgas pašvaldības sabiedrības ar ierobežotu atbildību „Rīgas satiksme” (turpmāk – Pasūtītājs) Iepirkuma komisija no iespējamā pretendenta ir saņēmusi lūgumu sniegt atbildes uz jautājumiem par iepirkuma procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) (turpmāk – iepirkuma procedūra) nolikuma prasībām.

1.jautājums
Vēlamies precizējumus par atklāta konkursa “Autobusu piegāde” Identifikācijas Nr.: RS/2026/17. 
Ņemot vērā, ka sistēmas ir identiskas, tad šie jautājumi attiecas uz: 
- 18m elektroautobusiem; 
- 18m dīzeļu autobusiem. 
Jautājums par tehniskās specifikācijas 9.2.1.1. punktu 
Lūdzam precizēt tehniskās specifikācijas 9.2.1.1. punktā noteiktās prasības attiecībā uz ārējiem LED informācijas paneļiem. 
Specifikācijā ir noteikts, ka priekšējam un sānu informācijas panelim jānodrošina divas teksta rindas ar burtu augstumu vismaz 100 mm, kā arī trīs simbolu maršruta numurs ar augstumu vismaz 140 mm. 
Vienlaikus sānu informācijas panelim ir noteikts minimālais attēlošanas laukums 160 × 900 mm. 
Lūdzam precizēt, kā šī prasība ir interpretējama, jo sānu panelī ar 160 mm augstumu fiziski nav iespējams attēlot divas teksta rindas, katru ar burtu augstumu vismaz 100 mm. Šādu attēlojumu iespējams nodrošināt priekšējam panelim, kura minimālais augstums ir 220 mm, taču ne sānu panelim. 
Vēlamies norādīt, ka autobūves nozarē ierasta prakse ir priekšējam informācijas panelim izmantot maksimāli lielus simbolus, lai maršruta numurs un galamērķis būtu skaidri saskatāmi no lielāka attāluma. Savukārt sānu panelī, ņemot vērā tā mazāko augstumu un atšķirīgo pielietojumu, parasti tiek izmantots nedaudz mazāks burtu augstums, vienlaikus saglabājot labu salasāmību pasažieriem pieturvietās. 
Lai novērstu minēto pretrunu un nodrošinātu tehniski realizējamu risinājumu, piedāvājam precizēt prasību, nosakot, ka sānu informācijas panelī ir pieļaujamas divas teksta rindas ar burtu augstumu vismaz 80 mm katrā rindā, savukārt priekšējam panelim saglabājama prasība par vismaz 100 mm augstiem burtiem. 
Šāds precizējums ir būtisks, lai korekti izstrādātu transportlīdzekļa komunikāciju tīkla arhitektūru un nodrošinātu atbilstību tehniskās specifikācijas prasībām.


Atbilde:
Pasūtītājs skaidro, ka iepirkuma procedūras Nolikuma Tehniskās specifikācijā noteicošais ir 9.2.1.1. punkta 3)apakšpunkts par LED paneļu minimālo attēlošanas laukumu ar norādīto minimālo izšķirtspēju pikseļos. Sānu paneļa atbilstība vērtējama pēc precizētajām prasībām par minimālo attēlošanas laukumu (160 × 900 mm) un izšķirtspēju (22 × 95 pikseļi). Attiecīgi Pretendents var ietvert risinājumu ar lielākiem izmēriem. Simbolu augstums nav atsevišķs atbilstības kritērijs sānu panelim.
Pasūtītājs vērš uzmanību, ka saskaņā ar ir 9.2.1.1. punkta 3) apakšpunkta noteikto Pretendents var piedāvāt funkcionāli ekvivalentu risinājumus, taču tādā gadījumā Pretendents nodrošina attiecīgo informāciju (pierādījumus), kas apliecina funkcionāli ekvivalentu risinājumu.



Iepirkuma komisijas priekšsēdētāja vietniece
										L. Hodaseviča 




11.08.2026.


Regarding the requirements of the open procedure "Supply of buses" (ID No RS 2026/17)

Riga Municipality Limited Liability Company (SIA) Rīgas satiksme (hereinafter – the Contracting Authority) has received a request from a potential Tenderer to provide answers to questions concerning the requirements of the Regulations of the open procedure "Supply of buses" (ID No RS 2026/17) (hereinafter – the procurement procedure).

Question 1
We would like to request clarifications regarding the open tender “Supply of Buses”, Identification No. RS/2026/17.
Considering that the systems are identical, these questions apply to:
· 18 m battery-electric buses;
· 18 m diesel buses.
Question regarding Section 9.2.1.1 of the Technical Specification
We kindly request clarification of the requirements set out in Section 9.2.1.1 of the Technical Specification regarding the external LED destination displays.
The specification states that the front and side destination displays shall provide two lines of text with a character height of at least 100 mm, as well as a three-character route number with a height of at least 140 mm.
At the same time, a minimum display area of 160 × 900 mm is specified for the side destination display.
Please clarify how this requirement should be interpreted, as it is physically impossible to display two lines of text, each with a character height of at least 100 mm, on a side display with a height of 160 mm. Such a display arrangement can be achieved on the front display, for which the minimum height is 220 mm, but not on the side display.
We would like to point out that, in the bus manufacturing industry, it is common practice for the front destination display to use the largest possible characters so that the route number and destination are clearly visible from a greater distance. In contrast, due to its smaller height and different purpose, the side display usually uses a slightly smaller character height while maintaining good readability for passengers at bus stops.
In order to eliminate the above-mentioned inconsistency and ensure a technically feasible solution, we propose that the requirement be amended by allowing the side destination display to provide two lines of text with a character height of at least 80 mm in each line, while retaining the requirement for the front display to provide characters with a height of at least 100 mm.
Such clarification is essential in order to correctly design the vehicle communication network architecture and ensure compliance with the requirements of the Technical Specification.
(Translated from Latvian using the machine translation tool “Copilot”)

Answer: 
The Contracting Authority clarifies that, within the Technical Specification of the Procurement Regulations, the determining requirement is Sub-section 3) of Section 9.2.1.1 concerning the minimum display area of the LED displays and the specified minimum resolution in pixels. Compliance of the side display shall be assessed based on the clarified requirements regarding the minimum display area (160 × 900 mm) and resolution (22 × 95 pixels). Accordingly, the Tenderer may include a solution with larger dimensions. The character height is not a separate compliance criterion for the side display.
The Contracting Authority draws attention to the fact that, in accordance with Subparagraph 3) of Clause 9.2.1.1, the Tenderer may offer functionally equivalent solutions. In such case, the Tenderer shall provide the relevant information (evidence) demonstrating that the proposed solutions are functionally equivalent.



Deputy Chairperson of the Procurement Commission
										L. Hodaseviča
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