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Par iepirkumu procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) nolikuma prasībām

Rīgas pašvaldības sabiedrības ar ierobežotu atbildību „Rīgas satiksme” (turpmāk – Pasūtītājs) Iepirkuma komisija no iespējamā pretendenta ir saņēmusi lūgumu sniegt atbildes uz jautājumiem par iepirkuma procedūras “Autobusu piegāde” (ID Nr. RS 2026/17) (turpmāk – iepirkuma procedūra) nolikuma prasībām.

1.jautājums
Jautājumi par rezerves daļu un ekspluatācijas materiālu piegādi plānveida apkopēm garantijas periodā
Saskaņā ar Tehniskās specifikācijas C sadaļu Piegādātājam ir jānodrošina rezerves daļas, ekspluatācijas materiāli un apkopes materiāli, kas nepieciešami regulāru plānveida apkopju veikšanai visā garantijas periodā. Pretendents saprot, ka gadījumā, ja tiek piedāvāts pagarināts transportlīdzekļa garantijas periods (virs minimālā garantijas perioda), attiecīgi būtu jāpaplašina arī piegādājamo rezerves daļu, ekspluatācijas materiālu un apkopes materiālu apjoms.
Šajā sakarā Pretendents lūdz sniegt skaidrojumu par turpmāk minēto:
1. Lūdzu, apstipriniet, vai gadījumā, ja tiek piedāvāts pagarināts transportlīdzekļa garantijas periods, Piegādātājam iepirkuma dokumentācijā noteiktajā termiņā ir jāpiegādā visi ekspluatācijas materiāli un apkopes materiāli, kas nepieciešami plānveida apkopēm visā pagarinātajā garantijas periodā.
2. Vai Pasūtītājam ir zināms, ka noteiktiem apkopes materiāliem un ekspluatācijas materiāliem, tostarp, bet ne tikai, smērvielām, eļļām, hermētiķiem, gumijas komponentēm, filtriem un citiem materiāliem, kas ir jutīgi pret novecošanos, ir ražotāja noteikts ierobežots uzglabāšanas termiņš un tie var zaudēt savas īpašības ilgstošas uzglabāšanas laikā neatkarīgi no tā, vai tie tiek izmantoti?
3. Ņemot vērā, ka visas šādas detaļas un materiāli tiks uzglabāti Pasūtītāja noliktavā un Piegādātājam nebūs kontroles pār uzglabāšanas apstākļiem (temperatūra, mitrums, piesārņojums, krājumu rotācija, apstrādes procedūras utt.), lūdzu, apstipriniet, ka:
• Pasūtītājs uzņemsies atbildību par ražotāju noteikto uzglabāšanas prasību ievērošanu;
• Piegādātājs nebūs atbildīgs par materiālu un ekspluatācijas materiālu īpašību pasliktināšanos, ekspluatācijas īpašību zudumu, derīguma termiņa beigām vai samazinātu kalpošanas laiku, kas radies ilgstošas uzglabāšanas vai neatbilstošu uzglabāšanas apstākļu dēļ pēc to piegādes un pieņemšanas no Pasūtītāja puses.
1. Alternatīvi, vai Pasūtītājs apsvērtu iespēju atļaut ekspluatācijas materiālu un apkopes materiālu piegādi pa daļām atbilstoši plānveida apkopes intervāliem, tādējādi nodrošinot atbilstību ražotāju noteiktajiem uzglabāšanas termiņiem un novēršot materiālu kvalitātes pasliktināšanās risku ilgstošas uzglabāšanas laikā?
Pamatojums:
Šī skaidrojuma pieprasījuma mērķis ir nodrošināt, lai piegādātie apkopes materiāli visā garantijas periodā pilnībā atbilstu ražotāja specifikācijām un būtu piemēroti lietošanai. Prasība piegādāt visus ekspluatācijas materiālus līguma sākumā var radīt situācijas, kad noteikti produkti sasniedz ieteicamā uzglabāšanas termiņa beigas pirms to plānotās izmantošanas, īpaši gadījumos, kad Pretendents piedāvā pagarinātu garantijas periodu. Šādi apstākļi pēc materiālu piegādes un pieņemšanas no Pasūtītāja puses vairs nav Piegādātāja kontrolē. Tādēļ būtu pateicīgi par skaidrojumu attiecībā uz atbildības sadalījumu un iespēju veikt piegādes pa posmiem.
(Tulkots no angļu valodas izmantojot mašīntulkošanas rīku “Copilot”)

Atbilde
Pasūtītājs  skaidro, ka saskaņā ar Tehniskās specifikācijas C.2.1. punktu rezerves daļu, patērējamo materiālu un dabīgi dilstošo detaļu apjoms ir jānodrošina visam Pretendenta piedāvātajam transportlīdzekļa garantijas periodam.
Līdz ar to gadījumā, ja Pretendents piedāvā garantijas termiņu, kas pārsniedz minimāli prasīto garantijas periodu, rezerves daļu, patērējamo materiālu un dabīgi dilstošo detaļu apjoms ir attiecīgi jānodrošina visam piedāvātajam garantijas periodam.
Vienlaikus Pasūtītājs  ir informēts, ka atsevišķiem patēriņa materiāliem un apkopes materiāliem var būt ražotāja noteikts ierobežots uzglabāšanas termiņš. Tomēr Pasūtītājs neparedz mainīt Tehniskajā specifikācijā un Līguma projektā noteikto kārtību attiecībā uz šo materiālu piegādi.
Pēc materiālu un rezerves daļu pieņemšanas Pasūtītājs nodrošina to uzglabāšanu atbilstoši attiecīgo ražotāju noteiktajām prasībām. Piegādātājs nav atbildīgs par materiālu vai detaļu īpašību pasliktināšanos, derīguma termiņa iestāšanos vai ekspluatācijas īpašību samazināšanos pēc to nodošanas Pasūtītājam, ja šādi apstākļi nav radušies Piegādātāja piegādāto materiālu vai detaļu neatbilstības dēļ piegādes brīdī.
Pasūtītājs nepieļauj periodiskajām apkopēm paredzēto rezerves daļu, materiālu un patēriņa materiālu pakāpenisku piegādi.


2.jautājums
Par 9. Informācijas un komunikācijas aprīkojumu
Lūdzu, sniedziet skaidrojumu par šādiem jautājumiem saistībā ar LED maršruta informācijas displeju integrāciju ITxPT sistēmā:
1. Vai Pasūtītājs atļauj izmantot starpprogrammu (proxy application) atbilstoši dokumentam S04P01N03 – AIS Formal Requirements?
2. Vai ir pieļaujams, ka LED displeji sazinās ar starpprogrammu, izmantojot savu atvērto un dokumentēto TCP balstītu bināro protokolu, nevis MQTT klientu, kas uzstādīts tieši katrā displejā?
3. Vai Pasūtītājs paredz iespēju uzstādīt starpprogrammu savā borta iekārtā?
4. Ja paredzēts, ka starpprogramma darbojas Pasūtītāja iekārtā, lūdzu, sniedziet informāciju par: 
1. operētājsistēmu un pieejamo izpildes vidi;
2. pieejamajiem aparatūras un programmatūras resursiem;
3. lietojumprogrammu uzstādīšanas un atjaunināšanas procedūrām;
4. pieejamajām tīkla saskarnēm;
5. drošības prasībām.
5. Ja starpprogrammas uzstādīšana Pasūtītāja iekārtā nav iespējama, vai būtu pieļaujams darbināt starpprogrammu kontrolierī, kas tiek piegādāta kā LED displeju sistēmas sastāvdaļa?
6. Vai programmatūras starpprogramma, kas darbojas esošajā kontrolierī, tiktu uzskatīta par “starpniekierīci” specifikācijas izpratnē, vai arī šis ierobežojums attiecas tikai uz papildu aparatūras ierīcēm?
7. Vai katram LED displejam ir jādarbojas kā tiešam MQTT klientam, vai pietiek, ja centrālā PIS/starpprogramma darbojas kā MQTT klients un pārstāv visus displejus?
8. Kura ITxPT specifikācijas versija ir prasīta: 
1. S02/Linden specifikācijas;
2. S04 specifikācijas uz MQTT bāzes;
3. abas versijas savietojamības nolūkos?
9. Kuras ITxPT tēmas (topics) displeju sistēmai ir obligāti jāatbalsta? Jo īpaši, vai ir prasīta šāda tēma:
10. <root>/current_destination_display/text
11. Vai Pasūtītājs pieļauj standarta ITxPT datu struktūru paplašināšanu, izmantojot papildu laukus vai papildu tēmas (topics)?
12. Ja paplašinājumi ir pieļaujami, lūdzu, precizējiet: 
• vai papildu dati jāiekļauj standarta datu struktūrā;
• vai tie jāpublicē atsevišķā tēmā;
• kāda nosaukumtelpa (namespace) jāizmanto;
• kā jānodrošina paplašinājumu versiju pārvaldība.
13. Tēmas current_destination_display/text piemēra datu struktūrā ir ietverts:
JSON
1
{
2
"number": 653,
3
"name": [
4
{
5
"lang": "pol",
6
"text": "Dworzec Główny"
7
}
8
],
9
"alternativeText": [
10
{
11
"lang": "pol",
12
"text": "via Centrum"
13
}
14
],
15
"lineDesignation": [
16
{
17
"lang": "pol",
18
"text": "22B"
19
}
20
],
21
"typeOfAlternativeText": "VIA"
22
}
13. Norādītajā struktūrā nav ietverta nepārprotama informācija par transportlīdzekļa tipu vai piktogrammu. Lūdzu, norādiet, kā šī informācija būtu jāpārsūta.
14. Vai piktogramma būtu jāpārsūta, izmantojot symbolName lauku, displayKeys struktūru vai ar Pasūtītāju saskaņota paplašinājuma palīdzību?
Vai Pasūtītāja sistēma publicēs galīgo tekstu, kas jāattēlo katrā LED displejā, vai arī PIS/starpprogrammai pašai ir jāģenerē attēlojamais saturs, balstoties uz aktuālajiem reisa datiem?
Vai Pasūtītājs pieprasa, lai LED displeji, izmantojot MQTT, sniegtu atgriezenisko informāciju, piemēram: 
• savienojuma statusu;
• pašlaik attēloto saturu;
• komandu izpildes apstiprinājumu;
• spilgtuma līmeni;
• temperatūru;
• kļūdu kodus un bojājumu statusu?
15. Vai saturs priekšējam, sānu, aizmugures un papildu displejam redzes invalīdiem tiks publicēts atsevišķi, vai arī PIS/starpprogrammai pašai būs jāģenerē atbilstošs saturs katram displejam?
16. Kā displejiem jārīkojas šādās situācijās: 
• savienojuma zudums ar MQTT brokeri;
• TCP savienojuma zudums ar starpprogrammu;
• tukšas datu struktūras saņemšana;
• aktuālā attēlojamā satura neesamība;
• sistēmas restartēšana?
17. Kurš ir atbildīgs par MQTT brokera nodrošināšanu un tā konfigurāciju, tostarp sertifikātiem, autentifikācijas datiem un ACL noteikumiem?
Kādi testi un pieņemšanas kritēriji tiks piemēroti, lai pārbaudītu risinājuma atbilstību ITxPT prasībām?
Vai ir kādas papildu ITxPT atbilstības, savietojamības, sertifikācijas vai pieņemšanas prasības, kas būtu jāņem vērā LED displeju sistēmas projektēšanas un ieviešanas laikā?
Pamatojums:
Šī skaidrojuma pieprasījuma mērķis ir nodrošināt piedāvātās pasažieru informēšanas sistēmas atbilstību Pasūtītāja ITxPT prasībām, vienlaikus saglabājot risinājuma savietojamību, kiberdrošību un ilgtermiņa uzturamību.
Šo aspektu precizēšana palīdzēs novērst integrācijas riskus, nodrošināt savietojamību ar Pasūtītāja borta sistēmām un ļaus visiem Pretendentiem sagatavot tehniski līdzvērtīgus un pilnībā prasībām atbilstošus risinājumus.
(Tulkots no angļu valodas izmantojot mašīntulkošanas rīku “Copilot”)

Atbilde:
Atbildes uz jautājumiem tiks sniegtas ne vēlāk kā līdz 2026.gada 12.augustam (ieskaitot).




Iepirkuma komisijas priekšsēdētāja vietniece
										L. Hodaseviča




11.08.2026.


Regarding the requirements of the open procedure "Supply of buses" (ID No RS 2026/17)

Riga Municipality Limited Liability Company (SIA) Rīgas satiksme (hereinafter – the Contracting Authority) has received a request from a potential Tenderer to provide answers to questions concerning the requirements of the Regulations of the open procedure "Supply of buses" (ID No RS 2026/17) (hereinafter – the procurement procedure).

Question 1
 Questions regarding the supply of spare parts and consumables for scheduled maintenance during the warranty period
According to Section C of the Technical Specification, the Supplier is required to provide spare parts, consumables and maintenance materials necessary for regular scheduled maintenance throughout the warranty period. The Tenderer understands that if an extended vehicle warranty is offered (beyond the minimum warranty period), the scope of spare parts, consumables and maintenance materials to be supplied should also be extended accordingly.

In this regard, the Tenderer kindly requests clarification of the following:

1. Please confirm whether, in the event of offering an extended vehicle warranty period, the Supplier is required to deliver, at the time specified in the procurement documentation, all consumables and maintenance materials required for scheduled maintenance covering the entire extended warranty period.
2. Is the Contracting Authority aware that certain maintenance materials and consumables, including but not limited to lubricants, greases, sealing compounds, rubber components, filters and other age-sensitive materials, have limited shelf life specified by their manufacturers and may deteriorate during long-term storage regardless of whether they are used?
3. Considering that all such parts and materials are to be stored in the Contracting Authority's warehouse and the Supplier has no control over storage conditions (temperature, humidity, contamination, stock rotation, handling procedures, etc.), please confirm that:

· the Contracting Authority will assume responsibility for ensuring compliance with the storage conditions prescribed by the manufacturers;
· the Supplier shall not be held liable for deterioration, loss of performance, expiration or reduced service life of materials and consumables resulting from prolonged storage or inappropriate storage conditions after delivery and acceptance by the Contracting Authority.
4. Alternatively, would the Contracting Authority consider allowing the delivery of consumables and maintenance materials in batches corresponding to the scheduled maintenance intervals, thereby ensuring compliance with manufacturers' shelf-life requirements and avoiding the risk of material degradation during long-term storage?
Justification:
The purpose of this clarification request is to ensure that the delivered maintenance materials remain fully compliant with manufacturers' specifications and fit for use throughout the entire warranty period. Requiring delivery of all consumables at the beginning of the contract may result in situations where certain products reach the end of their recommended storage life before their planned use, particularly in cases where the Tenderer offers an extended warranty period. Such circumstances are outside the Supplier's control once the materials have been delivered and accepted by the Contracting Authority. Therefore, clarification of the allocation of responsibility and the possibility of phased deliveries would be appreciated.


Answer 
The Contracting Authority explains that, in accordance with Clause C.2.1 of the Technical Specification, the quantity of spare parts, consumables and wear-and-tear components shall be sufficient for the entire vehicle warranty period offered by the Tenderer.
Accordingly, where a Tenderer offers a warranty period exceeding the minimum required warranty period, the quantity of spare parts, consumables and wear-and-tear components shall be increased accordingly to cover the entire warranty period offered.
At the same time, the Contracting Authority is informed that certain consumables and maintenance materials may be subject to manufacturer-specified limitations regarding storage life. However, the Contracting Authority does not intend to amend the delivery arrangements set out in the Technical Specification and draft of the Contract in respect of such materials.
Following acceptance of the materials and spare parts, the Contracting Authority shall ensure that they are stored in accordance with the requirements specified by the respective manufacturers. The Supplier shall not be liable for deterioration of material or component properties, expiry of shelf life, or reduction in performance characteristics occurring after delivery and acceptance by the Contracting Authority, provided that such circumstances do not result from non-conformity of the materials or components supplied by the Supplier at the time of delivery.
The Contracting Authority does not intend to permit phased deliveries of spare parts, materials and consumables intended for scheduled maintenance.



Question 2
Questions regarding 9. Information and communication equipment. 
Please clarify the following questions regarding the integration of LED destination displays with the ITxPT system:
1. Does the Contracting Authority allow the use of a proxy application in accordance with document S04P01N03 – AIS Formal Requirements?
2. Is it acceptable for the LED displays to communicate with the proxy application via their own open and documented TCP-based binary protocol, without an MQTT client installed directly on each display?
3. Does the Contracting Authority foresee the possibility of installing the proxy application on its onboard device?
4. If the proxy application is expected to run on the Contracting Authority’s device, please provide information regarding:
1. the operating system and available runtime environment;
2. available hardware and software resources;
3. application installation and update procedures;
4. available network interfaces;
5. security requirements.
5. If installation of the proxy application on the Contracting Authority’s device is not possible, would it be acceptable to run the proxy application on the controller supplied as part of the LED display system?
6. Would a software-based proxy application running on an existing controller be considered an “intermediary device” within the meaning of the specification, or does this restriction apply only to additional hardware devices?
7. Is each LED display required to operate as a direct MQTT client, or is it sufficient for a central PIS/proxy application to act as the MQTT client and represent all displays?
8. Which version of the ITxPT specification is required?
8. S02/Linden specifications;
8. S04 specifications based on MQTT;
8. both versions for compatibility purposes?
1. Which ITxPT topics are mandatory for the display system to support? In particular, is the following topic required?
1. <root>/current_destination_display/text
1. Does the Contracting Authority permit extensions to standard ITxPT payloads through additional fields or the use of additional topics?
1. If extensions are permitted, please specify:
· whether additional data should be included within the standard payload;
· whether it should be published in a separate topic;
· which namespace should be used;
· how extension versioning should be handled.
13. The example payload for the current_destination_display/text topic contains:
JSON
1
{
2
"number": 653,
3
"name": [
4
{
5
"lang": "pol",
6
"text": "Dworzec Główny"
7
}
8
],
9
"alternativeText": [
10
{
11
"lang": "pol",
12
"text": "via Centrum"
13
}
14
],
15
"lineDesignation": [
16
{
17
"lang": "pol",
18
"text": "22B"
19
}
20
],
21
"typeOfAlternativeText": "VIA"
22
}
13. In the presented structure, there is no explicit information regarding the vehicle type or pictogram. Please indicate how this information should be transmitted.
14. Should the pictogram be transmitted using the symbolName field, the displayKeys structure, or through an extension agreed with the Contracting Authority?
· Will the Contracting Authority’s system publish the final text to be displayed on each LED display, or is the PIS/proxy application expected to generate the display content independently based on the current service/trip data?
· Does the Contracting Authority require the LED displays to provide feedback information via MQTT, such as:
· connection status;
· currently displayed content;
· command execution confirmation;
· brightness level;
· temperature;
· error codes and fault status?
15. Will the content for the front, side, rear and additional display for visually impaired passengers be published separately, or is the PIS/proxy application expected to generate the appropriate content for each display?
16. How should the displays behave in the following situations:
· loss of connection to the MQTT broker;
· loss of TCP connection to the proxy application;
· reception of an empty payload;
· absence of current display content;
· system restart?
13. Who is responsible for providing the MQTT broker and its configuration, including certificates, authentication credentials and ACL rules?
1. What tests and acceptance criteria will be applied to verify compliance of the solution with the ITxPT requirements?
1. Are there any additional ITxPT compliance, interoperability, certification or acceptance requirements that should be taken into account during the design and implementation of the LED display system?

Justification: 
The purpose of this clarification request is to ensure compliance of the proposed passenger information system with the Contracting Authority’s ITxPT requirements while maintaining interoperability, cybersecurity and long-term maintainability of the solution.
Clarification of these aspects will help avoid integration risks, ensure compatibility with the Contracting Authority’s onboard systems, and enable all Tenderers to prepare technically equivalent and fully compliant solutions.

Answer: 
Answers to the questions will be provided no later than 12 August 2026 (inclusive)



Deputy Chairperson of the Procurement Commission
										L. Hodaseviča
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