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APSTIPRINĀTS
ar 2026. gada 6. jūlija 
Iepirkuma komisijas lēmumu


GROZĪJUMI
atklāta konkursa “Autobusu piegāde”
 (identifikācijas Nr. RS/2026/17) nolikumā

[bookmark: _Hlk101530575]Pamatojoties uz atklāta konkursa “Autobusu piegāde”, identifikācijas Nr.RS/2026/17, Iepirkuma komisijas 2026. gada 6. jūlija  lēmumu, izdarīt atklāta konkursa “Autobusu piegāde”, identifikācijas Nr.RS/2026/17, nolikumā (turpmāk - nolikums) šādus grozījumus:


1.TEHNISKAJĀ SPECIFIKĀCIJĀ.

1.1. [bookmark: _Hlk232748399]Grozīt Nolikuma 3.1. pielikuma “Tehniskā specifikācija iepirkuma priekšmeta 1.daļā”  “A.VISPĀRĪGĀS PRASĪBAS” sadaļas 8.1.punktu un izteikt jaunā redakcijā: 
[bookmark: _Toc337413756][bookmark: _Toc338589076][bookmark: _Toc229384686]“8.1.Kāpumu pārvarēšana
Transportlīdzeklim ar pilnu masu jāspēj uzsākt kustību un turpināt braukšanu augšup pa ceļu ar vismaz 12% kāpumu, uzsākot braukšanu no jebkura šī ceļa punkta, bez riteņu garenslīdes vai sānslīdes.
Papildus transportlīdzeklim ar pilnu masu uz ceļa ar 2.5% kāpumu jāspēj uzturēt braukšanas ātrumu ne mazāku kā 50 km/h. Papildus transportlīdzeklim ar pilnu masu jāspēj pārvarēt kāpumu ar vismaz 25 % slīpumu, nodrošinot nepārtrauktu kustību bez piedziņas jaudas ierobežojumiem”

1.2. Grozīt Nolikuma 3.2. pielikuma “Tehniskā specifikācija iepirkuma priekšmeta 2.daļā”  “A.VISPĀRĪGĀS PRASĪBAS” sadaļas 7.1.punktu un izteikt jaunā redakcijā:
[bookmark: _Toc229384167]“7.1.Kāpumu pārvarēšana
Transportlīdzeklim ar pilnu masu jāspēj uzsākt kustību un turpināt braukšanu augšup pa ceļu ar vismaz 12% kāpumu, uzsākot braukšanu no jebkura šī ceļa punkta, bez riteņu garenslīdes vai sānslīdes.
Papildus transportlīdzeklim ar pilnu masu uz ceļa ar 2.5% kāpumu jāspēj uzturēt braukšanas ātrumu ne mazāku kā 50 km/h. Papildus transportlīdzeklim ar pilnu masu jāspēj pārvarēt kāpumu ar vismaz 25 % slīpumu, nodrošinot nepārtrauktu kustību bez piedziņas jaudas ierobežojumiem.”


1.3. Aizstāt visā nolikuma tekstā vārdus un ciparus “2026. gada 4. augusts” attiecīgajā locījumā ar vārdiem un cipariem “2026. gada 18. augusts” attiecīgajā locījumā. 

Iepirkumu komisijas priekšsēdētāja                                                                K. Meiberga

Approved
by a decision of the Procurement Commission
meeting on July 6, 2026


AMENDMENTS
to the Regulations of the Open Procedure “Supply of buses” 
(Identification Number RS/2026/17) 


Based on the decision of the Procurement Commission of July 6, 2026 of the open procedure “Supply of buses”, identification No. RS/2026/17, the following amendments shall be made to the regulations of the open procedure “Supply of buses”, identification No. RS/2026/17 (hereinafter referred to as the regulations):

1. TECHNICAL SPECIFICATION.

1.1. Amend Annex 3.1 “Technical Specification for Lot 1 of the subject of the procurement” Section A. “GENERAL REQUIREMENTS” Clause 8.1., and express it in the following wording:
[bookmark: _Toc229573316]“8.1.Overcoming gradients
A vehicle at its maximum permissible mass shall be capable of starting and continuing on a road with a gradient of at least 12% from any point on the gradient, without wheel slip or skidding.
In addition, the vehicle at its maximum permissible mass shall be capable of maintaining a speed of not less than 50 km/h on a gradient of 2.5%. In addition, the vehicle at its maximum permissible mass shall be capable of negotiating a gradient of at least 25% without any restriction on propulsion power.”

1.2. Amend Annex 3.2 “Technical Specification for Lot 2 of the subject of the procurement” Section A. “GENERAL REQUIREMENTS” Clause 7.1., and express it in the following wording:
[bookmark: _Toc229573234]“7.1.Overcoming gradients
A vehicle at its maximum permissible mass shall be capable of starting and continuing on a road with a gradient of at least 12% from any point on the gradient, without wheel slip or skidding.
In addition, the vehicle at its maximum permissible mass shall be capable of maintaining a speed of not less than 50 km/h on a gradient of 2.5%. In addition, the vehicle at its maximum permissible mass shall be capable of negotiating a gradient of at least 25% without any restriction on propulsion power.”

1.3. Replace words and numbers throughout the text of the bylaw “August 4, 2026” in the relevant fold with words and numbers “August 18, 2026” in the relevant fold.

Chairwoman of the Procurement Commission                                            K. Meiberga
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